### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:13.2 (WebPack) - O.61xd | Target Family: | Spartan3
OS Platform: | NT64 | Target Device: | xc3s400
Project ID (random number) | 8e70cb1fb2c84c808800046dc397839e.18573E04A6144EADAF8AB70019B4F55C.23 | Target Package: | pq208
Registration ID | __0_0_0 | Target Speed: | -4
Date Generated | 2013-12-27T13:59:18 | Tool Flow | ISE

User Environment
OS Name | Microsoft Windows 7 , 64-bit | OS Release | Service Pack 1 (build 7601)
CPU Name | Intel(R) Core(TM) i5-2450M CPU @ 2.50GHz | CPU Speed | 2494 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Comparators=10

- 10-bit comparator greatequal=4
- 10-bit comparator less=6

Counters=2

- 10-bit up counter=2

Registers=5

- Flip-Flops=5

MiscellaneousStatistics

- AGG_BONDED_IO=8
- AGG_IO=8
- AGG_SLICE=25
- NUM_4_INPUT_LUT=46
- NUM_BONDED_IOB=8
- NUM_BUFGMUX=2
- NUM_CYMUX=18
- NUM_DCM=1
- NUM_SLICEL=25
- NUM_SLICE_FF=25
- NUM_XOR=20

NetStatistics

- NumNets_Active=70
- NumNets_Gnd=1
- NumNets_Vcc=1
- NumNodesOfType_Active_CLKPIN=17
- NumNodesOfType_Active_CNTRLPIN=15
- NumNodesOfType_Active_DOUBLE=69
- NumNodesOfType_Active_DUMMY=151
- NumNodesOfType_Active_DUMMYBANK=2
- NumNodesOfType_Active_DUMMYESC=3
- NumNodesOfType_Active_GLOBAL=14
- NumNodesOfType_Active_HFULLHEX=1
- NumNodesOfType_Active_HUNIHEX=3
- NumNodesOfType_Active_INPUT=162
- NumNodesOfType_Active_IOBOUTPUT=3
- NumNodesOfType_Active_OMUX=69
- NumNodesOfType_Active_OUTPUT=59
- NumNodesOfType_Active_PREBXBY=3
- NumNodesOfType_Active_VFULLHEX=4
- NumNodesOfType_Active_VLONG=1
- NumNodesOfType_Active_VUNIHEX=5
- NumNodesOfType_Vcc_CNTRLPIN=2
- NumNodesOfType_Vcc_VCCOUT=1

SiteStatistics

- IOB-DIFFM=6
- IOB-DIFFS=2
- SLICEL-SLICEM=14

SiteSummary

- BUFGMUX=2
- BUFGMUX_GCLKMUX=2
- BUFGMUX_GCLK_BUFFER=2
- DCM=1
- DCM_DCM=1
- IOB=8
- IOB_INBUF=3
- IOB_ISELMUX=1
- IOB_OUTBUF=6
- IOB_PAD=8
- IOB_TSMUX_GND=1
- SLICEL=25
- SLICEL_CYMUXF=10
- SLICEL_CYMUXG=8
- SLICEL_F=24
- SLICEL_FFX=14
- SLICEL_FFY=11
- SLICEL_G=22
- SLICEL_GNDF=10
- SLICEL_GNDG=8
- SLICEL_XORF=10
- SLICEL_XORG=10

Configuration Data
BUFGMUX

- S=[S_INV:2] [S:0]

BUFGMUX_GCLKMUX

- DISABLE_ATTR=[LOW:2]
- S=[S_INV:2] [S:0]

DCM

- PSCLK=[PSCLK_INV:0] [PSCLK:1]
- PSEN=[PSEN_INV:0] [PSEN:1]
- PSINCDEC=[PSINCDEC:1] [PSINCDEC_INV:0]
- RST=[RST:1] [RST_INV:0]

DCM_DCM

- CLKDV_DIVIDE=[2:1]
- CLKOUT_PHASE_SHIFT=[NONE:1]
- CLK_FEEDBACK=[1X:1]
- DESKEW_ADJUST=[7:1]
- DFS_FREQUENCY_MODE=[LOW:1]
- DLL_FREQUENCY_MODE=[LOW:1]
- DUTY_CYCLE_CORRECTION=[TRUE:1]
- FACTORY_JF1=[0X80:1]
- FACTORY_JF2=[0X80:1]
- PSCLK=[PSCLK_INV:0] [PSCLK:1]
- PSEN=[PSEN_INV:0] [PSEN:1]
- PSINCDEC=[PSINCDEC:1] [PSINCDEC_INV:0]
- RST=[RST:1] [RST_INV:0]

IOB

- O1=[O1_INV:0] [O1:6]

IOB_ISELMUX

- 0=[0:1] [0_INV:0]
- S0=[S0:1] [S0_INV:0]

IOB_OFF1

- CK=[CK:1] [CK_INV:0]
- D=[D:1] [D_INV:0]
- LATCH_OR_FF=[FF:1]
- OFF1_INIT_ATTR=[INIT1:1]
- OFF1_SR_ATTR=[SRHIGH:1]
- OFFATTRBOX=[ASYNC:1]
- SR=[SR:0] [SR_INV:1]

IOB_OUTBUF

- IN=[IN_INV:0] [IN:6]

IOB_PAD

- DRIVEATTRBOX=[12:6]
- IOATTRBOX=[LVCMOS25:8]
- SLEW=[SLOW:6]

SLICEL

- BX=[BX_INV:0] [BX:2]
- BY=[BY:1] [BY_INV:0]
- CE=[CE:1] [CE_INV:0]
- CIN=[CIN_INV:0] [CIN:8]
- CLK=[CLK:15] [CLK_INV:0]
- SR=[SR:0] [SR_INV:14]

SLICEL_CYMUXF

- 0=[0:10] [0_INV:0]
- 1=[1_INV:0] [1:10]

SLICEL_CYMUXG

- 0=[0:8] [0_INV:0]

SLICEL_F5MUX

- S0=[S0:1] [S0_INV:0]

SLICEL_FFX

- CK=[CK:14] [CK_INV:0]
- D=[D:14] [D_INV:0]
- FFX_INIT_ATTR=[INIT0:12] [INIT1:2]
- FFX_SR_ATTR=[SRLOW:12] [SRHIGH:2]
- LATCH_OR_FF=[FF:14]
- SR=[SR:0] [SR_INV:14]
- SYNC_ATTR=[ASYNC:14]

SLICEL_FFY

- CE=[CE:1] [CE_INV:0]
- CK=[CK:11] [CK_INV:0]
- D=[D:11] [D_INV:0]
- FFY_INIT_ATTR=[INIT0:11]
- FFY_SR_ATTR=[SRLOW:11]
- LATCH_OR_FF=[FF:11]
- SR=[SR:0] [SR_INV:10]
- SYNC_ATTR=[ASYNC:11]

SLICEL_XORF

- 1=[1_INV:0] [1:10]

Pin Data
BUFGMUX

- I0=2
- O=2
- S=2

BUFGMUX_GCLKMUX

- I0=2
- OUT=2
- S=2

BUFGMUX_GCLK_BUFFER

- IN=2
- OUT=2

DCM

- CLK0=1
- CLKFB=1
- CLKFX=1
- CLKIN=1
- PSCLK=1
- PSEN=1
- PSINCDEC=1
- RST=1

DCM_DCM

- CLK0=1
- CLKFB=1
- CLKFX=1
- CLKIN=1
- PSCLK=1
- PSEN=1
- PSINCDEC=1
- RST=1

IOB

- I=3
- O1=6
- PAD=8

IOB_INBUF

- IN=3
- OUT=3

IOB_ISELMUX

- 0=1
- 1=1
- OUT=1
- S0=1

IOB_OFF1

- CK=1
- D=1
- Q=1
- SR=1

IOB_OUTBUF

- IN=6
- OUT=6

IOB_PAD

- PAD=8

IOB_TSMUX_GND

- 0=1

SLICEL

- BX=2
- BY=1
- CE=1
- CIN=8
- CLK=15
- COUT=8
- F1=24
- F2=24
- F3=15
- F4=13
- G1=22
- G2=22
- G3=14
- G4=11
- SR=14
- X=10
- XQ=14
- Y=12
- YQ=11

SLICEL_CYMUXF

- 0=10
- 1=10
- OUT=10
- S0=10

SLICEL_CYMUXG

- 0=8
- 1=8
- OUT=8
- S0=8

SLICEL_F

- A1=24
- A2=24
- A3=15
- A4=13
- D=24

SLICEL_F5MUX

- F=1
- G=1
- OUT=1
- S0=1

SLICEL_FFX

- CK=14
- D=14
- Q=14
- SR=14

SLICEL_FFY

- CE=1
- CK=11
- D=11
- Q=11
- SR=10

SLICEL_G

- A1=22
- A2=22
- A3=14
- A4=11
- D=22

SLICEL_GNDF

- 0=10

SLICEL_GNDG

- 0=8

SLICEL_XORF

- 0=10
- 1=10
- O=10

SLICEL_XORG

- 0=10
- 1=10
- O=10

Tool Usage
Command Line History

- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- fuse

Software Quality
Run Statistics
Program Name | Runs Started | Runs Finished | Errors | Fatal Errors | Internal Errors | Exceptions | Core Dumps
_impact | 20 | 9 | 0 | 0 | 0 | 0 | 0
arwz | 7 | 7 | 0 | 0 | 0 | 0 | 0
bitgen | 211 | 211 | 0 | 0 | 0 | 0 | 0
cse_server | 7 | 6 | 0 | 0 | 0 | 0 | 0
edif2ngd | 2 | 2 | 0 | 0 | 0 | 0 | 0
map | 218 | 216 | 0 | 0 | 0 | 0 | 0
ngcbuild | 13 | 13 | 0 | 0 | 0 | 0 | 0
ngdbuild | 224 | 223 | 0 | 0 | 0 | 0 | 0
obngc | 2 | 2 | 0 | 0 | 0 | 0 | 0
par | 216 | 211 | 4 | 0 | 0 | 0 | 0
partgen | 29 | 27 | 0 | 0 | 0 | 0 | 0
trce | 207 | 207 | 0 | 0 | 0 | 0 | 0
xst | 342 | 342 | 0 | 0 | 0 | 0 | 0

Project Statistics
PROP_Enable_Message_Filtering=false | PROP_FitterReportFormat=HTML
PROP_LastAppliedGoal=Balanced | PROP_LastAppliedStrategy=Xilinx Default (unlocked)
PROP_ManualCompileOrderImp=false | PROP_PropSpecInProjFile=Store all values
PROP_SelectedInstanceHierarchicalPath=/TEST_BENCH | PROP_Simulator=ISim (VHDL/Verilog)
PROP_SynthTopFile=changed | PROP_Top_Level_Module_Type=HDL
PROP_UseSmartGuide=false | PROP_UserConstraintEditorPreference=Text Editor
PROP_UserEditorCustomSetting={C:\Program Files (x86)\Notepad++\\Notepad++} $1 | PROP_UserEditorPreference=Custom
PROP_intProjectCreationTimestamp=2013-12-23T22:38:22 | PROP_intWbtProjectID=18573E04A6144EADAF8AB70019B4F55C
PROP_intWbtProjectIteration=23 | PROP_intWorkingDirLocWRTProjDir=Same
PROP_intWorkingDirUsed=No | PROP_lockPinsUcfFile=changed
PROP_selectedSimRootSourceNode_behav=work.TEST_BENCH | PROP_AutoTop=true
PROP_DevFamily=Spartan3 | PROP_DevDevice=xc3s400
PROP_DevFamilyPMName=spartan3 | PROP_DevPackage=pq208
PROP_Synthesis_Tool=XST (VHDL/Verilog) | PROP_DevSpeed=-4
PROP_PreferredLanguage=VHDL | FILE_UCF=1
FILE_VHDL=2 | FILE_XAW=1

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=2 | NGDBUILD_NUM_DCM=1 | NGDBUILD_NUM_FDC=22 | NGDBUILD_NUM_FDE=1
NGDBUILD_NUM_FDP=2 | NGDBUILD_NUM_GND=1 | NGDBUILD_NUM_IBUF=2 | NGDBUILD_NUM_IBUFG=1
NGDBUILD_NUM_INV=1 | NGDBUILD_NUM_LUT2=12 | NGDBUILD_NUM_LUT2_D=1 | NGDBUILD_NUM_LUT2_L=2
NGDBUILD_NUM_LUT3=6 | NGDBUILD_NUM_LUT3_L=1 | NGDBUILD_NUM_LUT4=20 | NGDBUILD_NUM_LUT4_D=2
NGDBUILD_NUM_LUT4_L=2 | NGDBUILD_NUM_MUXCY=18 | NGDBUILD_NUM_OBUF=6 | NGDBUILD_NUM_XORCY=20
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=2 | NGDBUILD_NUM_DCM=1 | NGDBUILD_NUM_FDC=22 | NGDBUILD_NUM_FDE=1
NGDBUILD_NUM_FDP=2 | NGDBUILD_NUM_GND=1 | NGDBUILD_NUM_IBUF=2 | NGDBUILD_NUM_IBUFG=1
NGDBUILD_NUM_INV=1 | NGDBUILD_NUM_LUT2=12 | NGDBUILD_NUM_LUT2_D=1 | NGDBUILD_NUM_LUT2_L=2
NGDBUILD_NUM_LUT3=6 | NGDBUILD_NUM_LUT3_L=1 | NGDBUILD_NUM_LUT4=20 | NGDBUILD_NUM_LUT4_D=2
NGDBUILD_NUM_LUT4_L=2 | NGDBUILD_NUM_MUXCY=18 | NGDBUILD_NUM_OBUF=6 | NGDBUILD_NUM_XORCY=20

XST Command Line Options
XST_OPTION_SUMMARY
-ifn=<fname>.prj | -ifmt=mixed | -ofn=<design_top> | -ofmt=NGC
-p=xc3s400-4-pq208 | -top=<design_top> | -opt_mode=Speed | -opt_level=1
-iuc=NO | -keep_hierarchy=No | -netlist_hierarchy=As_Optimized | -rtlview=Yes
-glob_opt=AllClockNets | -read_cores=YES | -write_timing_constraints=NO | -cross_clock_analysis=NO
-bus_delimiter=<> | -slice_utilization_ratio=100 | -bram_utilization_ratio=100 | -verilog2001=YES
-fsm_extract=YES | -fsm_encoding=Auto | -safe_implementation=No | -fsm_style=LUT
-ram_extract=Yes | -ram_style=Auto | -rom_extract=Yes | -shreg_extract=YES
-rom_style=Auto | -auto_bram_packing=NO | -resource_sharing=YES | -async_to_sync=NO
-mult_style=Auto | -iobuf=YES | -max_fanout=500 | -bufg=8
-register_duplication=YES | -register_balancing=No | -optimize_primitives=NO | -use_clock_enable=Yes
-use_sync_set=Yes | -use_sync_reset=Yes | -iob=Auto | -equivalent_register_removal=YES
-slice_utilization_ratio_maxmargin=5

ISim Statistics
Xilinx HDL Libraries Used=ieee, unisim, std
Fuse Resource Usage=982 ms, 47084 KB
Total Signals=268
Total Nets=261
Total Blocks=23
Total Processes=96
Total Simulation Time=86111937500 ps
Simulation Resource Usage=87.6102 sec, 478511 KB
Simulation Mode=gui
Hardware CoSim=0