### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:13.1 (WebPack) - O.40d | Target Family: | Spartan3
OS Platform: | NT64 | Target Device: | xc3s400
Project ID (random number) | fdea62e8f41646f59dc0337c9f5daf2b.46EAA90106E94458A48103B48AC9CA6F.10 | Target Package: | pq208
Registration ID | _ | Target Speed: | -4
Date Generated | 2014-02-28T15:52:03 | Tool Flow | ISE

User Environment
OS Name | Microsoft Windows 7 , 64-bit | OS Release | Service Pack 1 (build 7601)
CPU Name | Intel(R) Core(TM) i5-2450M CPU @ 2.50GHz | CPU Speed | 2494 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Adders/Subtractors=2

- 20-bit adder=2

Counters=3

- 26-bit up counter=1
- 4-bit up counter=2

FSMs=1 Multiplexers=1

- 1-bit 12-to-1 multiplexer=1

Registers=81

- Flip-Flops=81

MiscellaneousStatistics

- AGG_BONDED_IO=3
- AGG_IO=3
- AGG_SLICE=92
- NUM_4_INPUT_LUT=137
- NUM_BONDED_IOB=3
- NUM_BUFGMUX=1
- NUM_CYMUX=51
- NUM_LUT_RT=44
- NUM_SLICEL=92
- NUM_SLICE_FF=92
- NUM_XOR=46

NetStatistics

- NumNets_Active=180
- NumNets_Gnd=1
- NumNets_Vcc=1
- NumNodesOfType_Active_CLKPIN=64
- NumNodesOfType_Active_CNTRLPIN=78
- NumNodesOfType_Active_DOUBLE=234
- NumNodesOfType_Active_DUMMY=318
- NumNodesOfType_Active_DUMMYESC=1
- NumNodesOfType_Active_GLOBAL=19
- NumNodesOfType_Active_HUNIHEX=2
- NumNodesOfType_Active_INPUT=367
- NumNodesOfType_Active_IOBOUTPUT=1
- NumNodesOfType_Active_OMUX=214
- NumNodesOfType_Active_OUTPUT=175
- NumNodesOfType_Active_PREBXBY=22
- NumNodesOfType_Active_VFULLHEX=13
- NumNodesOfType_Active_VLONG=1
- NumNodesOfType_Active_VUNIHEX=6
- NumNodesOfType_Gnd_DOUBLE=2
- NumNodesOfType_Gnd_INPUT=2
- NumNodesOfType_Gnd_OMUX=2
- NumNodesOfType_Gnd_OUTPUT=2
- NumNodesOfType_Gnd_PREBXBY=2

SiteStatistics

- IOB-DIFFM=2
- IOB-DIFFS=1
- SLICEL-SLICEM=55

SiteSummary

- BUFGMUX=1
- BUFGMUX_GCLKMUX=1
- BUFGMUX_GCLK_BUFFER=1
- IOB=3
- IOB_INBUF=2
- IOB_OUTBUF=1
- IOB_PAD=3
- SLICEL=92
- SLICEL_C1VDD=2
- SLICEL_CYMUXF=27
- SLICEL_CYMUXG=24
- SLICEL_F=63
- SLICEL_F5MUX=2
- SLICEL_F6MUX=1
- SLICEL_FFX=32
- SLICEL_FFY=60
- SLICEL_G=74
- SLICEL_GNDF=25
- SLICEL_GNDG=24
- SLICEL_XORF=23
- SLICEL_XORG=23

Configuration Data
BUFGMUX

- S=[S_INV:1] [S:0]

BUFGMUX_GCLKMUX

- DISABLE_ATTR=[LOW:1]
- S=[S_INV:1] [S:0]

IOB

- O1=[O1_INV:0] [O1:1]

IOB_OUTBUF

- IN=[IN_INV:0] [IN:1]

IOB_PAD

- DRIVEATTRBOX=[12:1]
- IOATTRBOX=[LVCMOS25:3]
- SLEW=[SLOW:1]

SLICEL

- BX=[BX_INV:1] [BX:8]
- BY=[BY:16] [BY_INV:0]
- CE=[CE:21] [CE_INV:0]
- CIN=[CIN_INV:0] [CIN:24]
- CLK=[CLK:64] [CLK_INV:0]
- SR=[SR:44] [SR_INV:13]

SLICEL_CYMUXF

- 0=[0:27] [0_INV:0]
- 1=[1_INV:0] [1:27]

SLICEL_CYMUXG

- 0=[0:24] [0_INV:0]

SLICEL_F5MUX

- S0=[S0:2] [S0_INV:0]

SLICEL_F6MUX

- S0=[S0:1] [S0_INV:0]

SLICEL_FFX

- CE=[CE:18] [CE_INV:0]
- CK=[CK:32] [CK_INV:0]
- D=[D:31] [D_INV:1]
- FFX_INIT_ATTR=[INIT0:28] [INIT1:4]
- FFX_SR_ATTR=[SRLOW:28] [SRHIGH:4]
- LATCH_OR_FF=[FF:32]
- SR=[SR:17] [SR_INV:12]
- SYNC_ATTR=[ASYNC:3] [SYNC:29]

SLICEL_FFY

- CE=[CE:21] [CE_INV:0]
- CK=[CK:60] [CK_INV:0]
- D=[D:60] [D_INV:0]
- FFY_INIT_ATTR=[INIT0:54] [INIT1:6]
- FFY_SR_ATTR=[SRLOW:43] [SRHIGH:17]
- LATCH_OR_FF=[FF:60]
- SR=[SR:41] [SR_INV:12]
- SYNC_ATTR=[ASYNC:7] [SYNC:53]

SLICEL_XORF

- 1=[1_INV:0] [1:23]

Pin Data
BUFGMUX

- I0=1
- O=1
- S=1

BUFGMUX_GCLKMUX

- I0=1
- OUT=1
- S=1

BUFGMUX_GCLK_BUFFER

- IN=1
- OUT=1

IOB

- I=2
- O1=1
- PAD=3

IOB_INBUF

- IN=2
- OUT=2

IOB_OUTBUF

- IN=1
- OUT=1

IOB_PAD

- PAD=3

SLICEL

- BX=9
- BY=16
- CE=21
- CIN=24
- CLK=64
- COUT=24
- F1=63
- F2=40
- F3=25
- F4=19
- F5=2
- FXINA=1
- FXINB=1
- G1=74
- G2=51
- G3=27
- G4=18
- SR=57
- X=29
- XB=1
- XQ=32
- Y=26
- YQ=60

SLICEL_C1VDD

- 1=2

SLICEL_CYMUXF

- 0=27
- 1=27
- OUT=27
- S0=27

SLICEL_CYMUXG

- 0=24
- 1=24
- OUT=24
- S0=24

SLICEL_F

- A1=63
- A2=40
- A3=25
- A4=19
- D=63

SLICEL_F5MUX

- F=2
- G=2
- OUT=2
- S0=2

SLICEL_F6MUX

- 0=1
- 1=1
- OUT=1
- S0=1

SLICEL_FFX

- CE=18
- CK=32
- D=32
- Q=32
- SR=29

SLICEL_FFY

- CE=21
- CK=60
- D=60
- Q=60
- SR=53

SLICEL_G

- A1=74
- A2=51
- A3=27
- A4=18
- D=74

SLICEL_GNDF

- 0=25

SLICEL_GNDG

- 0=24

SLICEL_XORF

- 0=23
- 1=23
- O=23

SLICEL_XORG

- 0=23
- 1=23
- O=23

Tool Usage
Command Line History

- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -i -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s400-pq208-4 <ise_file> <fname>.ngd
- map -intstyle ise -p xc3s400-pq208-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd

Software Quality
Run Statistics
_impact | 10 | 3 | 0 | 0 | 0 | 0 | 0
bitgen | 15 | 15 | 0 | 0 | 0 | 0 | 0
cse_server | 8 | 8 | 0 | 0 | 0 | 0 | 0
edif2ngd | 4 | 4 | 0 | 0 | 0 | 0 | 0
elfcheck | 2 | 2 | 0 | 0 | 0 | 0 | 0
libgen | 4 | 4 | 0 | 0 | 0 | 0 | 0
map | 18 | 18 | 0 | 0 | 0 | 0 | 0
netgen | 15 | 15 | 0 | 0 | 0 | 0 | 0
ngcbuild | 27 | 27 | 0 | 0 | 0 | 0 | 0
ngdbuild | 18 | 18 | 0 | 0 | 0 | 0 | 0
obngc | 6 | 6 | 0 | 0 | 0 | 0 | 0
par | 17 | 15 | 2 | 0 | 0 | 0 | 0
partgen | 26 | 25 | 0 | 0 | 0 | 0 | 0
platgen | 1 | 1 | 0 | 0 | 0 | 0 | 0
psf2Edward | 1 | 1 | 0 | 0 | 0 | 0 | 0
trce | 15 | 15 | 0 | 0 | 0 | 0 | 0
xdsgen | 1 | 1 | 0 | 0 | 0 | 0 | 0
xps | 2 | 2 | 0 | 0 | 0 | 0 | 0
xst | 69 | 68 | 0 | 0 | 0 | 0 | 0

Project Statistics
PROP_Enable_Message_Filtering=false | PROP_FitterReportFormat=HTML
PROP_LastAppliedGoal=Balanced | PROP_LastAppliedStrategy=Xilinx Default (unlocked)
PROP_ManualCompileOrderImp=false | PROP_PropSpecInProjFile=Store all values
PROP_Simulator=ISim (VHDL/Verilog) | PROP_SynthTopFile=changed
PROP_Top_Level_Module_Type=HDL | PROP_UseSmartGuide=false
PROP_UserConstraintEditorPreference=Text Editor | PROP_intProjectCreationTimestamp=2013-11-24T21:28:59
PROP_intWbtProjectID=46EAA90106E94458A48103B48AC9CA6F | PROP_intWbtProjectIteration=10
PROP_intWorkingDirLocWRTProjDir=Same | PROP_intWorkingDirUsed=No
PROP_lockPinsUcfFile=changed | PROP_AutoTop=false
PROP_DevFamily=Spartan3 | PROP_DevDevice=xc3s400
PROP_DevFamilyPMName=spartan3 | PROP_DevPackage=pq208
PROP_Synthesis_Tool=XST (VHDL/Verilog) | PROP_DevSpeed=-4
PROP_PreferredLanguage=VHDL | FILE_UCF=1
FILE_VHDL=2

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUFGP=1 | NGDBUILD_NUM_FD=1 | NGDBUILD_NUM_FDE=9 | NGDBUILD_NUM_FDR=31
NGDBUILD_NUM_FDRE=30 | NGDBUILD_NUM_FDS=21 | NGDBUILD_NUM_GND=1 | NGDBUILD_NUM_INV=4
NGDBUILD_NUM_LUT1=44 | NGDBUILD_NUM_LUT2=38 | NGDBUILD_NUM_LUT2_L=1 | NGDBUILD_NUM_LUT3=13
NGDBUILD_NUM_LUT3_L=2 | NGDBUILD_NUM_LUT4=27 | NGDBUILD_NUM_LUT4_D=6 | NGDBUILD_NUM_LUT4_L=4
NGDBUILD_NUM_MUXCY=51 | NGDBUILD_NUM_MUXF5=2 | NGDBUILD_NUM_MUXF6=1 | NGDBUILD_NUM_OBUF=1
NGDBUILD_NUM_VCC=1 | NGDBUILD_NUM_XORCY=46
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=1 | NGDBUILD_NUM_FD=1 | NGDBUILD_NUM_FDE=9 | NGDBUILD_NUM_FDR=31
NGDBUILD_NUM_FDRE=30 | NGDBUILD_NUM_FDS=21 | NGDBUILD_NUM_GND=1 | NGDBUILD_NUM_IBUF=1
NGDBUILD_NUM_IBUFG=1 | NGDBUILD_NUM_INV=4 | NGDBUILD_NUM_LUT1=44 | NGDBUILD_NUM_LUT2=38
NGDBUILD_NUM_LUT2_L=1 | NGDBUILD_NUM_LUT3=13 | NGDBUILD_NUM_LUT3_L=2 | NGDBUILD_NUM_LUT4=27
NGDBUILD_NUM_LUT4_D=6 | NGDBUILD_NUM_LUT4_L=4 | NGDBUILD_NUM_MUXCY=51 | NGDBUILD_NUM_MUXF5=2
NGDBUILD_NUM_MUXF6=1 | NGDBUILD_NUM_OBUF=1 | NGDBUILD_NUM_VCC=1 | NGDBUILD_NUM_XORCY=46