VERSION:3 SOURCE_TIMESTAMP:51796EFC
NODE:I LEVEL:0 LINE:1 "C:\cvavr\inc\mega16.h"
NODE:I LEVEL:0 LINE:2 "C:\cvavr\inc\string.h"
NODE:I LEVEL:0 LINE:3 "C:\cvavr\inc\alcd.h"
NODE:M LEVEL:0 LINE:7 "DATA_REGISTER_EMPTY"
NODE:M LEVEL:0 LINE:8 "RX_COMPLETE"
NODE:M LEVEL:0 LINE:9 "FRAMING_ERROR"
NODE:M LEVEL:0 LINE:10 "PARITY_ERROR"
NODE:M LEVEL:0 LINE:11 "DATA_OVERRUN"
NODE:M LEVEL:0 LINE:14 "RX_BUFFER_SIZE"
NODE:V LEVEL:0 LINE:15 "rx_buffer -> RAM:????"
NODE:V LEVEL:0 LINE:18 "rx_wr_index -> R5"
NODE:V LEVEL:0 LINE:18 "rx_rd_index -> R4"
NODE:V LEVEL:0 LINE:24 "rx_counter -> R7"
NODE:V LEVEL:0 LINE:30 "rx_buffer_overflow -> R2.0"
NODE:V LEVEL:0 LINE:32 "mDotFlag -> R6"
NODE:V LEVEL:0 LINE:33 "mNCount -> R9"
NODE:V LEVEL:0 LINE:34 "mInReceive -> R8"
NODE:F LEVEL:0 LINE:38 "usart_rx_isr(void)"
NODE:I LEVEL:0 LINE:67 "C:\cvavr\inc\stdio.h"
NODE:C LEVEL:0 LINE:70 "AT_CMT -> FLASH"
NODE:F LEVEL:0 LINE:72 "main(void)"
