Protel Design System Design Rule Check
PCB File : D:\Latif\023\EKH023PCB001(Control)_BGA\EKH023PCB001.PcbDoc
Date     : 09/10/2014
Time     : 04:20:07 È.Ù

Processing Rule : Differential Pairs Uncoupled Length using the Gap Constraints (Min=0.15mm) (Max=0.15mm) (Preferred=0.15mm)  and Width Constraints (Min=0.075mm) (Max=0.381mm) (Preferred=0.075mm) (All)
   Violation between Differential Pairs Routing Between Net CK_2_P And Net CK_2_N
Rule Violations :1

Processing Rule : Width Constraint (Min=0.075mm) (Max=3mm) (Preferred=0.075mm) (All)
Rule Violations :0

Processing Rule : Differential Pairs Uncoupled Length using the Gap Constraints (Min=0.15mm) (Max=0.15mm) (Preferred=0.15mm)  and Width Constraints (Min=0.075mm) (Max=0.381mm) (Preferred=0.075mm) (InDifferentialPair ('L32') Or InDifferentialPair ('L15') Or InDifferentialPair ('DATA') Or InDifferentialPair ('UDQS_2') Or InDifferentialPair ('L63') Or InDifferentialPair ('L17') Or InDifferentialPair ('L16') Or InDifferentialPair ('UDQS') Or InDifferentialPair ('L64') Or InDifferentialPair ('HIGH PERFORMANCE OS') Or InDifferentialPair ('L33') Or InDifferentialPair ('L66') Or InDifferentialPair ('L49') Or InDifferentialPair ('L14') Or InDifferentialPair ('L38') Or InDifferentialPair ('L51') Or InDifferentialPair ('L3') Or InDifferentialPair ('DATA_C') Or InDifferentialPair ('L6') Or InDifferentialPair ('LDQS_2') Or InDifferentialPair ('L50') Or InDifferentialPair ('L44') Or InDifferentialPair ('L18') Or InDifferentialPair ('L48') Or InDifferentialPair ('L46') Or InDifferentialPair ('L5') Or InDifferentialPair ('L43') Or InDifferentialPair ('L8') Or InDifferentialPair ('L4') Or InDifferentialPair ('L62') Or InDifferentialPair ('L2') Or InDifferentialPair ('CK') Or InDifferentialPair ('L47') Or InDifferentialPair ('CK_2') Or InDifferentialPair ('L7') Or InDifferentialPair ('LDQS') Or InDifferentialPair ('L45'))
Rule Violations :0

Processing Rule : Width Constraint (Min=0.075mm) (Max=3mm) (Preferred=0.075mm) (InDifferentialPair('L32') Or InDifferentialPair('L15') Or InDifferentialPair('DATA') Or InDifferentialPair('UDQS_2') Or InDifferentialPair('L63') Or InDifferentialPair('L17') Or InDifferentialPair('L16') Or InDifferentialPair('UDQS') Or InDifferentialPair('L64') Or InDifferentialPair('HIGH PERFORMANCE OS') Or InDifferentialPair('L33') Or InDifferentialPair('L66') Or InDifferentialPair('L49') Or InDifferentialPair('L14') Or InDifferentialPair('L38') Or InDifferentialPair('L51') Or InDifferentialPair('L3') Or InDifferentialPair('DATA_C') Or InDifferentialPair('L6') Or InDifferentialPair('LDQS_2') Or InDifferentialPair('L50') Or InDifferentialPair('L44') Or InDifferentialPair('L18') Or InDifferentialPair('L48') Or InDifferentialPair('L46') Or InDifferentialPair('L5') Or InDifferentialPair('L43') Or InDifferentialPair('L8') Or InDifferentialPair('L4') Or InDifferentialPair('L62') Or InDifferentialPair('L2') Or InDifferentialPair('CK') Or InDifferentialPair('L47') Or InDifferentialPair('CK_2') Or InDifferentialPair('L7') Or InDifferentialPair('LDQS') Or InDifferentialPair('L45'))
Rule Violations :0

Processing Rule : Short-Circuit Constraint (Allowed=No) (All),(All)
Rule Violations :0

Processing Rule : Un-Routed Net Constraint ( (All) )
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.1mm) (All),(All)
Rule Violations :0

Processing Rule : Power Plane Connect Rule(Direct Connect )(Expansion=0.508mm) (Conductor Width=0.254mm) (Air Gap=0.254mm) (Entries=4) (All)
Rule Violations :0

Processing Rule : Width Constraint (Min=0.075mm) (Max=6mm) (Preferred=0.075mm) (All)
Rule Violations :0

Processing Rule : Routing Via (MinHoleWidth=0.2mm) (MaxHoleWidth=1mm) (PreferredHoleWidth=0.25mm) (MinWidth=0.4mm) (MaxWidth=2mm) (PreferedWidth=0.45mm) (All)
Rule Violations :0

Processing Rule : Component Clearance Constraint ( Horizontal Gap = 0.254mm, Vertical Gap = 0.254mm ) (Disabled)(All),(All) 
Rule Violations :0

Processing Rule : Hole Size Constraint (Min=0.2mm) (Max=5mm) (All)
Rule Violations :0

Processing Rule : Hole To Hole Clearance (Gap=0.15mm) (All),(All)
Rule Violations :0

Processing Rule : Net Antennae (Tolerance=0mm) (All)
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=1mm) (OnLayer('SIG1') OR OnLayer('SIG2') OR OnLayer('SIG3') OR OnLayer('SIG4')),((INPolygon))
Rule Violations :0

Processing Rule : Differential Pairs Uncoupled Length using the Gap Constraints (Min=0.15mm) (Max=0.15mm) (Preferred=0.15mm)  and Width Constraints (Min=0.381mm) (Max=0.381mm) (Preferred=0.381mm) (All)
Rule Violations :0

Processing Rule : Width Constraint (Min=0.075mm) (Max=3mm) (Preferred=0.075mm) (InDifferentialPair('UDQS') Or InDifferentialPair('LDQS_2') Or InDifferentialPair('LDQS') Or InDifferentialPair('CK') Or InDifferentialPair('UDQS_2') Or InDifferentialPair('CK_2'))
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.4mm) (OnLayer('Top Layer') OR OnLayer('Bottom Layer')),((INPolygon))
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.2mm) (OnLayer('GND1') OR OnLayer('GND2') OR OnLayer('GND3') OR OnLayer('GND4') OR OnLayer('GND5') OR OnLayer('GND6')),(All)
Rule Violations :0


Violations Detected : 1
Time Elapsed        : 00:00:42